List of low-cost energy-saving measures at 27 Aston Street
The only things we have done that aren’t low cost are:
1. Installing thermal water-heating panels on the roof.  This was done in 2007, costing £7,000, so I cannot say what they would cost now.

2. Fitting UPVC double-glazed windows in four rooms upstairs – necessitated by the construction of the Conservatory, which prevented all those windows from being able to be cleaned outside from a ladder.
Downstairs front room
· Dry-lining the front bay window
· Fitting foil behind the radiator (supplied by LCEO Robin)
· Having the two side windows in the bay draughtproofed professionally – the rep advised us not to do anything to the front windows as they were painted shut.
· Commissioning thermal linings for the new curtains
Front hall
· Fitting a panel inside the top front window, above the door, as this showed up as losing more heat on the thermal imaging study.
Kitchen
· Fitting a Perspex panel outside the main window – detachable when the weather warms up
· Using a draught excluder snake between the kitchen and Conservatory
Conservatory
· Fitting foil behind the radiators (supplied by LCEO Robin) – but note that this room is not normally used/heated in the colder months
Upstairs front bedroom
· Commissioning thermal linings for the curtains
· Fitting foil behind the radiator (supplied by LCEO Robin)
Back bedroom
Dry-lining an exposed wall in the north facing room.  Along with the double-glazing, this has been extremely effective, and the room barely needs heating.
